;=?>< OPERA

TION REPOR

T Ver.1.5

93 B 5 C 13 A Y+ 82 KSC @D: GI : FE:JH

E0102 ! Lynx-Field

P ASS 1 P

ASS 2 P

ASS 3 P

ASS 4 P

ASS 5

Pass No. 930513{0412 930513{0516 930513{0619 930513{0723 930513{0826

Operation X-Rep

OPOG-WR T

OP-ST AR T

X-Rep

RANG

ST-CTLG-WR T

OBS-MODE

S-Rep

BDR-STOP

S-REP

BDR-STOP

X-REP X-Rep

T arget

E0102 E0102 E0102 E0102

Lynx Field

AOS(UT) 5:57:50 7:39:43 9:20:56 11:02:57 12:44:43

LOS(UT) 6:09:58 7:51:58 9:33:44 11:15:20 12:56:29

Max-El 16.47 49.638 Zenith 70.298 26.254

Time 6:03:54 7:45:14 | 11:08:33 12:49:58

Rep-band X X S X X

Rep-start 5:59:57 7:40:25 9:21:51/9:27:34 11:03:42 12:45:46

Rep-status Completed Completed Interrupted COMPLETE Completed

DP-mode OBS OBS/ACS/OBS OBS OBS OBS

ACS-mode Normal{Poin ting Normal{Poin ting Normal{Pointing Normal{Pointing Normal{Pointing

ACS-spn/�

s 3:5

�

3:5

�

3:6

�

3.6

�

18.4

�

Attitude

2

4

15.857

162.205

58.397

3

5

2

4

15.857

162.204

16058.397

3

5

2

4

15.857

162.204

58.397

3

5

2

4

15.858

162.204

58.398

3

5

2

4

132.786

44.928

171.727

3

5

OP-start 6:07:01 contin ue continue Cont. Cont.

start CE 60h 07h 0Eh 17h 24h

SIS-mode

Fnt/Fn t

1CCD

F ant/F an t

1CCD

F ant/F ant

1CCD

F ant/F ant

1CCD

F ant/F ant

4CCD

S0/1-TECT �40:70= � 40:65 �40:12= � 40:11 �39:39= � 39:48 �38:76= � 38:85 �38:42= � 38:56

S0/1-CCDT �61:71= � 61:81 �61:76= � 61:86 �61:76= � 61:86 �61:71= � 61:81 �61:71= � 61:81

GIS-mode

PH MES PH MES PH MES PH MES PH MES

GIS LD Hit 24cps/21cps 29cps/26cps 30cps/32cps 30cps/30cps 29cps/28cps

P X Y R S Pos MErr HV HL Gain RT-L RT-U T emp RBMT CalPk RT Pk CalCnt/time

10 8 8 5 0 FLF

| 3/4 48 159 218 12.5 12.5 414.0 183.8 1808cts

Pass: s9305130412 3/4

40 159 218 7.1 428.8 181.9 1889cts

GIS Mo de Changes: no

Battery Condition (min/max)

BA T V{A BA

T V{B BA

T I{A BA

T I{B BA

T T{A BA

T T{B Charge/Discharge

20.20/23.40 20.30/23.50 �4.16/4.73 �4.43/4.76 4.82/8.74 4.82/8.46 no go o d data

Comment: KN09L"

MNV INFORMA

TION SCHEDULED IN THE OP COMMANDS

MNV ST AR T: 5/13 12:25:00,T AR GET:Lynx �eld,(�; � )=(133.30,44.84),Euler Angle:(132.68,45.08,171.86)

F rom the sum of 5/12 data and 5/13 data, we got E0102-72 sp ectrum of 3.6 ksec exp osure for b oth SIS

and GIS. F rom the SIS sp ectrum, we can resolve prominent 0.9 keV and 1.0 keV lines in the cluster of F e

L-shell lines. The structure due to F e L-shell lines and Mg line is also visible in the sp ectrum of GIS. After

the 4th pass, ASCA was maneuvered to the Lynx �eld.

QN1 U_W TY ‘ E0102 8b ,$2 )*! RN &50 X#W -Ma ’c ’6 GIS 0 VZT Y^ /41+ (6 \

S_.P%740’b%2)*!

][#Y0d3&5 Lynx �eld 100ksec 0ef/O62)*!