BDFEC OPERA

TION REPOR

T Ver.1.5

93 I 5 J 14 H Y+ 83 KSC GK: NP, ML A QO

Lynx-Field

P ASS 1 P

ASS 2 P

ASS 3 P

ASS 4 P

ASS 5

Pass No. 930514{0412 930514{0516 930514{0619 930514{0723 930514{0826

Operation X-Rep

OPOG-WR T

01-F

AINT

OP-ST AR T

X-Rep

RANG

X-Rep

BDR-STOP

X-REP

BDR-STOP

GIS-CPU-S2/3

STOP

,RESET

X-REP

RANG

X-Rep

T arget Lynx-Field Lynx-Field Lynx-Field Lynx-�eld Lynx Field

AOS(UT) 5:56:56 7:39:10 9:20:29 11:02:38 12:44:20

LOS(UT) 6:09:48 7:51:31 9:33:12 11:14:44 12:55:28

Max-El 23.389 63.346 Zenith 56.660 18.722

Time 6:03:19 7:44:15 | 11:08:05 12:49:24

Rep-band X X X X X

Rep-start 5:58:55 7:39:53 9:21:27/9:27:17 11:03:19 12:45:29

Rep-status Completed Completed Interrupted Completed Completed

DP-mode OBS OBS OBS OBS OBS

ACS-mode Normal{Poin ting Normal{Poin ting Normal{Pointing Normal{Pointing Normal{Pointing

ACS-spn/�

s 19:1

�

19:2

�

19:2

�

19.3

�

19.3

�

Attitude

2

4

132.671

45.067

171.848

3

5

2

4

132.671

45.067

171.848

3

5

2

4

132.672

45.067

171.848

3

5

2

4

132.671

45.067

171.848

3

5

2

4

132.671

45.067

171.848

3

5

OP-start 6:06:47 contin ue continue Cont. Cont.

start CE 00h 07h 0Eh 17h 1Eh

SIS-mode

Brt-Fnt/Brt-Fn t

4CCD

F ant/F an t

4CCD

F ant/F ant

4CCD

F ant/F ant

4CCD

F ant/F ant

4CCD

S0/1-TECT �41:81= � 41:67 �41:28= � 41:03 �40:70= � 40:50 �40:21= � 40:01 �40:02= � 39:77

S0/1-CCDT �61:76= � 61:86 �61:81= � 61:86 �61:76= � 61:86 �61:76= � 61:86 �61:76= � 61:86

GIS-mode

PH MES PH MES PH MES PH MES PH MES

GIS LD Hit 24cps/26cps 27cps/31cps 30cps/31cps 31cps/30cps 27cps/26cps

P X Y R S Pos MErr HV HL Gain RT-L RT-U T emp RBMT CalPk RT Pk CalCnt/time

10 8 8 5 0 FLF

| 3/4 48 159 218 12.5 12.5 418.56 183.84 2978cts

Pass: s9305140412 3/4

40 159 218 7.1 435.82 182.38 2963cts

GIS Mo de Changes: no

Battery Condition (min/max)

BA T V{A BA

T V{B BA

T I{A BA

T I{B BA

T T{A BA

T T{B Charge/Discharge

20.30/23.40 20.30/23.50 �4.12/4.73 �4.43/4.76 4.82/8.74 4.82/8.46 no go o d data

Comment: RV5?S"

Lynx �eld. Nothing a source in the GIS image of ab out 10 ksec exp osure. Beutifully(?) empty and at

image due to mostly cosmic X-ray background and partly contaminated by non-X-ray background. GIS count

rate is ab out 0.5 counts/sec/GIS(s2+s3) for accumulation of all photons within the region encircled by R =

86 ch ( = 2.1 cm) in the image. Contamination of the installed calibration source is visible at 6.4 keV in the

GIS sp ectrum.

ZV6 Lynx-�eld 5 ]^ = Y3/ -![ V5 E0102 5 ‘d *U T/- ]^ 1b 9; 1 Z V5 ]^ 6 i5 \4 _ el6m3(/-$Wok>a%!:’pVhX,0@(c(8n)<7 g&5.+<2!

q#!$jf%